04/21/2023 iain Galloway [iain.galloway@nxp.com](mailto:iain.galloway@nxp.com)Notes from email conversation between board house and designer:  
-=-=-=-  
In the FMUM-RT1172 FAB DWG, the instruction shows 10 layers.   
However, in the Gerber file, there are only 8 layers. It looks like layer 5 & 6 are missing.

You are correct! These layers were absent from the gerbers. I have regenerated the gerbers with these layers included. Please see the attached zip. My apologies for the mixup.